**Non-Contact Vital Sign Monitoring**

**Introduction**

Although vital signs provide critical information in determining a patient’s current state of health,

they are not always measurable using conventional methods [1]. For infants, elderly, or patients suffering

from burns, health care providers experience difficulty continuously measuring the blood pressure,

temperature, respiration rate, or heart rate of patients, which can identify the existence of an acute medical

condition, help to rapidly quantify the magnitude of an illness, and act as a marker of chronic disease

states [2]. As a result, researchers and health care providers developed ways to measure vital signs

without invasive contact with the patient’s body. This paper is a review of technologies associated with

methods currently utilized to provide non-contact vital sign monitoring and the impact these technologies

would have in patient care globally.

**Camera-Based Non-Contact Vital Sign Monitoring**

Since the 1930s, it has been known that the variations in tissue blood volume in a body segment,

with each heartbeat, modulate the transmission of visible light through or from that body segment [3].

This light transmission or reflectance is known as the photoplethysmographic (PPG) signal, which can be

utilized to measure the heart rate, respiration rate, and blood oxygen level of a patient [3,4]. Recently,

researchers have been able to accurately measure the PPG signal of subjects with a digital video camera

up to two meters away from the subject, using only ambient light as the light source [3].

Researchers at Rice University were able to determine the heart rate of a subject using a

monochrome camera and a PPG estimation algorithm they developed by measuring the change of

hemoglobin and oxyhemoglobin in any area of a subject’s face [4]. Although the study needs more data to

prove that this method is viable for long-term monitoring, the results, with respect to the technology used

to conduct the study, are promising. With the average cost of a monochrome camera ranging from $7,000

to over $40,000 in an age where the price of technology decreases rapidly as new technology is

developed, this technology could replace the monitoring equipment in hospitals that range from $20,000

to $30,000 per setup [5,6].

**Under-the-Bed Noncontact Sensors**

With elderly care and long-time monitoring as customer requirements to measure vital signs,

muRata, an electronics company, developed an accelerometer-based ballistocardiographic (BCG) signal

sensor that is attached under a patient’s bed to measure vital signs continuously [4]. It works by capturing

the vibrations on the bed caused by a patient’s heart rate, respiration, and body movement using an ultra-

sensitive accelerometer and using a microcontroller to process the information and produce the

measurements [4]. The solution includes a PCB module that contains the accelerometer and the

microcontroller for BCG algorithm processing and it also includes a PCB module with the bonus of WiFi

connectivity for ease of integration [7,8]. The modules are sold in units with prices ranging from $106.82

to $137.84 per unit for the PCB module and $170.92 to $198.88 per unit for the PCB module with WiFi

according to prices listed on Digi-Key’s site.

**Doppler/Radar Non-Contact Vital Sign Monitoring**

Microwave Doppler radar has gained popularity in wireless sensing applications, including

volume change sensing, life detection, and cardiopulmonary monitoring, which has propelled in interest

in non-contact vital sign monitoring [9]. The Doppler radar first transmits a radio-frequency continuous

wave quadrature signal captures the signal once it has been reflected off of the human body []. After the

signal is amplified and down-converted, the signal is phase modulated by the physiological movements,

and then the human heartbeat and respiration rates are identified by processing the baseband signal using

advanced signal processing techniques [9]. A biomedical company, SENSIOTEC, has developed an

Impulse Radio Ultra-Wideband sensor using this technology, but it is not widely available due to

expensive and specialized hardware [4,10].

**The Potential Impact of Implementation**

The impact of the implementation of non-contact vital sign monitoring technology expands across

homes and industries globally. The implementation of this technology will protect infants in the Neonatal

Intensive Care Unit (NICU), who often suffer from skin damage as a result of requiring electrodes,

adhesive tapes, other probes to continuously measure vitals, but it could also protect infants in their

homes by helping to prevent Sudden Infant Death Syndrome (SIDS) [4,10]. This technology can also

provide health care aid in third world countries where supplies are limited and risk of disease or infection

is increased. Car manufacturers are also interested in utilizing this technology to prevent accidents caused

by drivers that are sleepy, under the influence, or suffering from seizures or heart attacks [11].

**Bibliography**

[1] Troy Madison, “Why Vital Signs are Important for ER Doctors,” University of Utah Health, 16-

Jun-2017.

[2] C. Goldberg, “A Practical Guide to Clinical Medicine,” A Practical Guide to Clinical Medicine.

[Online]. Available: https://meded.ucsd.edu/clinicalmed/vital.htm. [Accessed: 20-Oct-2018].

[3] L. Tarassenko, M. Villarroel, A. Guazzi, J. Jorge, D. A. Clifton, and C. Pugh, “Non-contact

video-based vital sign monitoring using ambient light and auto-regressive models,” Physiological

Measurement, vol. 35, no. 5, pp. 807–831, Mar. 2014.

[4] T. Hall, D. Lie, T. Nguyen, J. Mayeda, P. Lie, J. Lopez, and R. Banister, “Non-Contact Sensor for

Long-Term Continuous Vital Signs Monitoring: A Review on Intelligent Phased-Array Doppler

Sensor Design,” Sensors, vol. 17, no. 11, p. 2632, Nov. 2017.

[5] “Monochrome Digital Camera,” Gear, DPP MAG, 04-May-2015.

[6] J. Lagasse, “Continuous monitoring tools could save hospitals $20,000 per bed, report

says,” Healthcare IT News, 28-Jun-2017. [Online]. Available:

https://www.healthcareitnews.com/news/continuous-monitoring-tools-could-save-hospitals-

20000-bed-report-says. [Accessed: 20-Oct-2018].

[7] muRata, SCA10H Datasheet, Sep. 2015 [Revised Aug. 2016].

[8] muRata, SCA11H Datasheet, Sep. 2015 [Revised Dec. 2015].

[9] C. Li, J. Ling, J. Li, and J. Lin, “Accurate Doppler Radar Noncontact Vital Sign Detection Using

*the RELAX Algorithm,” IEEE Transactions on Instrumentation and Measurement, vol. 59, no. 3,*

pp. 687–695, Mar. 2010.

[10] F. Zhao, M. Li, Z. Jiang, J. Z. Tsien, and Z. Lu, “Camera-Based, Non-Contact, Vital-Signs

Monitoring Technology May Provide a Way for the Early Prevention of SIDS in

Infants,” Frontiers in Neurology, vol. 7, Dec. 2016.

[11] “Five benefits of non-contact vital sign monitoring which make it one to watch in

2014,” Oxehealth, 17-Feb-2014. [Online]. Available: https://www.oxehealth.com/news/five-

benefits-non-contact-vital-sign-monitoring-make-one-watch-2014. [Accessed: 20-Oct-2018].